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ENGINEERING CHANGE ORDER
	
REV A



1. GENERAL INFORMATION
	ALT Model #:
	BFX-AT100
	*Effective Date:
	2024/9/1

	ODM Information

	Name of ODM:
	Foxconn
	
	

	Submitted date:
	2024/8/5
	Submitted By:
	Cato Chang

	
	
	Email:
	Cato.yn.chang@fii-foxconn.com


*Effective date: production begins with this ECO.

2. Hardware or Component Changes
	From
	Old part(s)
	To
	New part(s)

	No.
	ODM P/N
	Manufacture
	Ordering code
	Part ref
	ODM P/N
	Manufacture
	Ordering code
	*IC

	1
For example:
	NA
	TI
	TPS25200DRVR
	U308
	NA
	AWINIC
	AW35019DNR
	B

	
	Part description:
	IC SW 2.5~6.5V SMD WSON6 GP/HF TPS25200DRVR
	IC SW 2.5~6.5V SMD WSON6 GP/HF AW35019DNR

	2
	NA
	VISHAY
	TSOP75338TR
	U402
	NA
	Everlight
	IRM-V838J12-S/TR1(KU)(HFX)
	B

	
	Part description:
	IR RECEIVER 38KHz SMD SMD4 GP/HF TSOP75338TR
	IR RECEIVER 38KHz SMD SMD4 GP/HF IRM-V838J12-S/TR1(KU)(HFX)

	3
	NA
	TI
	TLV75518PDBVR
	U303
U306
	NA
	ETA-semi
	ETA5056V18S2F
	B

	
	Part description:
	IC REG 1.8V 500mA SMD SOT23-5 GP TLV75518PDBVR
	IC REG 1.8V 500mA SMD SOT23-5 GP ETA5056V18S2F　

	4
	NA
	TI
	TLV75525PDBVR
	U307
	NA
	ETA-semi
	ETA5056V25S2F
	B

	
	Part description:
	IC REG 2.5V 500mA SMD SOT23-5 GP/HF TLV75525PDBVR
	IC REG 1.8V 500mA SMD SOT23-5 GP ETA5056V25S2F　

	5
	NA
	POWERWAY
	MPTFP2-V-TR

	SW901
SW902
SW401
	NA
	POWERWAY
	ST39-NPM20-B3RQ-L
	B

	
	Part description:
	SW TACT 50mA 12V SMD ST GP/HF
	SW TACT 50mA 12V SMD ST GP/HF

	6
	NA
	AMAZING
	AZ1065-06F.R7G

	D901
	NA
	APM
	AR0506PAL
	B

	
	Part description:
	DIODE ESD ARRAY 6V 0.0025mA SMD DFN4120P
	DIODE ESD ARRAY 6V 0.0025mA SMD DFN4120P

	7
	NA
	HOSONIC
	E3SB25.0000F12NGY
	Y801
	NA
	Faith Long
	3S250F1057
	B

	
	Part description:
	XTAL 25MHz 7ppm 12pF 50ohm SMD GP/HF 3.2

	XTAL 25MHz 7ppm 12pF 50ohm SMD GP/HF 3.2


	8
	NA
	HOSONIC
	E2SB20E00000XE
	Y1001
	NA
	Faith Long
	2S200F1002
	B

	
	Part description:
	XTAL 20MHz 20ppm 8pF 50ohm SMD GP/HF 2.5
	XTAL 20MHz 20ppm 8pF 50ohm SMD GP/HF 2.5

	Affected Units:
	Affected Processes:

	Affected all units of this model
	Affected units within the range
	Production
	Service only

	EAGLE
	TBC, Fii will provide the SN we start to implement 2nd source later.
	EAGLE only
	NA

	*IC (Interchangeability Code) defined:

	A
	The new part is a drop-in replacement; it is 100% interchangeable with the old part both functionally and mechanically. 
For production, no longer be used old part. For example: running change. 

	B
	The new part is a drop-in replacement; it is 100% interchangeable with the old part both functionally and mechanically 
For production, may be used in both new and old part. For example: multi (alternative) parts.

	C
	The new part may be used in both new and old products. The old part can ONLY be used in old products

	D
	The old part should no longer be used. All existing stock must be purged.  Only the NEW part may be used

	E
	The parts are NOT interchangeable. Old parts must be used in old products and new parts must be used in new products


3. 
Reason for Change
	For example: The current “IR receiver”, p/n TSOP75338TR, used at U402 has gone End Of Life and no stock can be found.  The supporting manufacturer’s PCN is attached.

	First is for cost down
Then, In order to increase suppliers to meet normal supply and avoid material shortage problems



4. Reference Documents
	[bookmark: _Hlk173327326]Note: All relevant supporting documents must accompany the ECO in order for it to be approved. Otherwise, the ECO may be delayed or rejected.

	Component datasheets
With spec comparison sheet
(Old / New)
	Complete/Update schematics (with changes highlighted)
	Supporting Test Data
	PCN or manufacturer notification letter (EOL, Leadtime, etc)
	Other supporting documents (PCNs, etc)

	Please see the mantis 1176: ~  message, there are comparison table and datasheet in excel file
	Above parts are 2nd source, main source are still in use, there is no need to update schematic
	Please see the mantis 1176, all test report are uploaded on there.
	No EOL for these parts
	Fii will process the PCN internally once getting email form ALT to show us BMT is passed.



5. Cut-in information
	Note: Must be written based on customer S/N. If separated into multiple ranges, record all of the S/N ranges.

	For example.
Cut in S/N : 2149688001202499000010~
Cut in S/N : 2149688001202499000011 ~ 2149688001202499000020
TBC, Fii will provide the SN we start to implement 2nd source later.



6. For ALT use only
	Signoff:	Lonnie Kim

	Job Title
Name
Signature
Date:
	HW Leader

Lonnie Kim



2004/08/09
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