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2. BMT 의뢰서
2.1. HW 사양
	Chipset
	Amlogic S905X2

	Flash
	eMMC 8GB

	DRAM
	DDR4 3GB

	OS
	Android TV "Pie" ver

	Video Decoding
	H.264 BP/MP/HP@L4.x, H.265 HEVC MP/MP10@L5.1, 
VP9, MPEG4, MPEG2, MJPEG

	Audio Decoding
	AAC, HE-AAC, Dolby Digital Plus
MPEG-1 Audio Layer1, 2, 3
PCM(LPCM / ADPCM)


	Bluetooth
	BT4.2

	Front
	1 X LED (Red/Green/Blue)
1 X IR

	TOP
	2 X KEY (CH+/-)

	Rear
	1 X HDMI 2.0
1 X 10/100/1000 Base-T Ethernet 
1 X DC 5V/2A IN
1 X USB 3.0
1 X MIC Jack

	Power Supply
	5V/2A
















2.1. 1. Block diagram 
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2.1. 2. PCB Assay
a. Set-Top Main Board assy: TOP Side
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b. Set-Top Main Board assy: BOTTOM Side
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2.1.3. 제품 디자인 
(최종 렌더링 이미지는 10/19/금 제출 예정.)
- Front


- Rear 


- Left


- Right






- Top




- Bottom







2.1.4. Accessories
-HDMI cable *1
-Cat. 5e LAN cable *1
-User Manual *1
-5V/2A Adapter *1
-IR/BT RCU *1




2.1.5. Main Parts List
	Item
	PART DESCRIPTION
	Quantity

	1
	Audio ADC: IC DSP 3.6V SMD QFN24 8~96KHz GP/HF 
	1

	2
	BT: IC MPU 3.3V SMD FCBGA49 2.4GHz GP/HF
	1

	3
	GIGA Ethernet PHY: IC PER 1.5/1.8/2.5/3.3V SMD QFN40 GP ETHERNET TRANSCEIVER
	1

	4
	Main SOC: IC PER 1.8/3.3V SMD FCBGA393 GP ARM
	1

	5
	DDR4 8Gb: IC DDR4 SDRAM 8Gb 1.2V 0.625nS SMD FBGA96 GP
	2

	6
	EMMC 8GB: IC eMMC 8GB 2.7~3.6V 5nS SMD FBGA153 GP 
	1

	7
	IR: IR RECEIVER 38KHz SMD SMD4 GP
	1

	8
	Microphone Input: CONN AUDIO JACK 1*1PORT D=3.6/7.0mm DIP F RT GP
	1

	9
	USB 3.0: CONN USB 3.0 A 1*1PORT 2.0mm DIP F RT GP/HF
	1

	10
	HDMI: CONN HDMI A 19PIN 1*1PORT 0.5mm SMD MALE RT GP
	1

	11
	RJ-45: CONN RJ45 8P8C 1u"GOLD 1*1PORT W/LED Y/G 2.04mm DIP F RT GP BLACK
	1

	12
	DDR4 4Gb: IC DDR4 SDRAM 4Gb 1.2V 0.625nS SMD FBGA96 GP 
	2

	13
	DC Jack: CONN PWR JACK 1*1PORT D=2.0/6.5mm DIP FEMALE RT GP 5V 2A 
	1
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