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The purpose of this document is to ensure that results obtained from testing the product to the Acceptance Test Procedure (ATP) are captured along with all other relevant information such as software versions and equipment lists etc. This can then be used to show compliance to the Product Requirement Specification.
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This procedure should only be used for STB products and variants thereof, as the requirements are specific as declared in the Product SPEC.
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UUT data
	Date Test Completed
	2021/3/5

	Name of Eng./Tech. Performing Tests; Org/Dept
	Catherine Chen

	Model Name
	BFX-UA300
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	Item Number
	Description

	1
	BFX-UA300 4K Soundbar DUT

	2
	BT Remote Controller 

	3
	Monitor w/ HDMI port

	4
	AAA battery 2x
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· Test Step

1. Test location : office
Test environment setting : Box and RCU distance at least keep 15m
2. Box horizontal and vertical deflection at 0°, +/- 30°, +/- 45°…
3. Measure RCU each function key can work 0°, +/- 30°, +/- 45°…
4. Repeat step 2,3 and test all degree

[image: ]
Figure 5. Test diagram


· Test Result

Table 8. User Environment Test Result
	Measurement Positions
	Distance
	Actual Test Distance
	Result
	RCU key function

	Nearby 
	> 20cm
	> 50cm
	PASS
	Functional key:
Power on/off
Change channel key
TV key
Home key
Up/Down/Left/Right/OK key
Back key
Menu key
Vol. Up/Down key

	Front (0°)
	> 15m
	> 17m
	PASS
	

	Horizontal Deflection (+30°)
	
	
	PASS
	

	Horizontal Deflection (-30°)
	
	
	PASS
	

	Horizontal Deflection (+45°)
	
	
	PASS
	

	Horizontal Deflection (-45°)
	
	
	PASS
	

	Vertical Deflection (+30°)
	
	
	PASS
	

	Vertical Deflection (-30°)
	
	
	PASS
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